### Connect Network Cable

In order to configure the printer, it needs to be discovered on the network. Temporarily plugging in the network cable allows the printer to be discovered on the network and the installation to continue. Once the printer is configured for wireless communication, the setup wizard prompts you to remove the cable.

1. Do one of the following:

- Connect one end of the network cable to an available Ethernet port on your network.
- Connect one end of the cross cable (included with the printer) to your computer's Ethernet adapter.
  Caution: Do not connect the cross cable to the network Ethernet port.

2. Connect the other end of the cable to the network port on the back of the printer.
   Caution: Do not connect the cable to the USB or parallel port.

If the link light is... | Then...
On and green | Click Yes.
Off | o Verify that the cable is securely connected to both the printer and the network Ethernet port or computer. o Verify that the printer is turned on. o Verify that the computer is connected to the network.