|  | Setting and Referencing Device Information
| Setting the Device Password

This section describes the procedure for setting or changing a device's password. (This function can only be used with Canon devices.)
When a password is set for a device, the password must be input to perform the operations requiring administrator's privileges such as configuring protocol settings and device information. You can set a password for each device.

| The password set with NetSpot Device Installer for some devices may differ from the administrator password used on the operation panel of the unit or on Remote UI.
| It is recommended that you use a password that cannot be easily guessed by anyone other than the administrator.

1. In the device list, select the device, and then select [Change Password] from the [Device] menu.
   You can also select [Change Password] by right-clicking a device in the list (with a Macintosh, by clicking it while holding down the control key) and selecting the item from the menu displayed.
2. Set or change the password in the [Change Device Password] dialog box.

   | [Old password]: Input the password that is currently set for the device. If no password is set, leave this blank. [New password]: Input the new password to be set. [Confirm]: Input the new password a second time.

3. Click the [OK] button.

   | The new password is enabled.