|  | Setting and Referencing Device Information
| Referencing Port Information

This section describes how to reference device port (LPD, RAW, IPP) information. (This function can only be used with Canon devices.)

1. In the device list, select the device, and then select [TCP/IP Port Information] from the [Device] menu.
   You can also select [TCP/IP Port Information] by right-clicking a device in the list (with a Macintosh, by clicking it while holding down the control key) and selecting the item from the menu displayed.
2. Reference the information in the [TCP/IP Port Information] dialog box.

   | [Product Name]: The product name for the device. [Device Name]: The device name that you can reference or set in the [Device Name] field of the [Device Information] dialog box. [LPD]
   | [Status]: The current status of the LPD port. ([Enabled]: usable / [Disabled]: not usable)
   | [IP Address]: The IP address of the device.
   | [Port Name]: The LPD port name.
   [RAW]
   | [Status]: The current status of the RAW port. ([Enabled]: usable / [Disabled]: not usable)
   | [Port Number]: The RAW port number.
   | [Description]: Description of the RAW port.
   [IPP]
   | [Status]: The current status of the IP port. ([Enabled]: usable / [Disabled]: not usable)
   | [URI]: The URI of the IPP. The URI that is displayed begins with [http://] if the port number is 80, with [ipp://] if the port number is 631, and with [<IP address>:<port number>//] in all other cases.

   | Port information that is not supported by the model is left blank.

3. Click the [OK] button.

   | The dialog box closes.