  Microsoft Network Client 3.0 for MS-DOS
                  and
  Microsoft Windows for Workgroups 3.11

  Introduction:
  -------------
  This document describes the procedure to setup the Microsoft Network
  Client for DOS driver on D-Link DGE-528T Gigabit Ethernet Adapter.

  Location of Driver: \NDIS2\DOS\D528N2.DOS

  Sample Configuration Files:
  ---------------------------
  Ex1: [PROTOCOL.INI] (install creates this file)

  [network.setup]
  version=0x3110
  netcard=DGE-528T,1,DGE-528T,1
  transport=ms$ndishlp,MS$NDISHLP
  transport=ms$netbeui,MS$NETBEUI
  lana0=DGE-528T,1,ms$netbeui
  lana1=DGE-528T,1,ms$ndishlp

  [protman]
  DriverName=PROTMAN$
  PRIORITY=MS$NDISHLP

  [MS$NDISHLP]
  DriverName=ndishlp$
  BINDINGS=DGE-528T

  [MS$NETBEUI]
  DriverName=netbeui$
  SESSIONS=10
  NCBS=12
  BINDINGS=DGE-528T
  LANABASE=0


  [DGE-528T]
  ; DGE-528T RPOTOCOL.INI SAMPLE
  DriverName=D528N2$
  EtherID=@52544C111111 ;This keyword is used to desinate a DGE-528T
  ;adapter by assigning its ethernet ID
  ;when more than one adapters exist on one
  ; system.

  BusNo=@00 ;This keyword is used to desinate a DGE-528T
  ;adapter by assigning it's PCI bus number
  ;when more than one adapters exist on one
  ; system.(must be used with 'DeviceNo' keyword)

  DeviceNo=@0A ;This keyword is used to desinate a DGE-528T
  ;adapter by assigning it's PCI Device number
  ;when more than one adapters exist on one
  ; system.(must be used with 'BusNo' keyword)

  Medium= Auto ;This keyword is used to force DGE-528T adapter
  ;to speed 1000M,100M or 10M mode. If not present,
  ;the driver will auto-detect the speed. example:
  ;Auto --Auto negotiation
  ;100FULL --100M FullDuplex
  ;100Half --100M HalfDuplex
  ;10Full --10M FullDuplex
  ;10Half --10M HalfDuplex

  Installation Procedure:
  -----------------------
  Before you start with the installation procedure, make sure that the
  adapter is properly installed and configured. Similarly, Make sure
  that your Microsoft Network Client is properly installed.
  (If not, The installation utility SETUP.EXE is located on Microsoft
  Network Client v3.0 for MS-DOS Disk. Run SETUP.EXE from Disk and the
  SETUP program screen will appear, and You must complete each of the
  questions. These options are specific to your needs. The installation
  procedure will transfer files to a specific directory on the client
  and modify existing configuration files to fit your specific needs.)

  1. Change to the Microsoft Network Client subdirectory, and run
  SETUP.EXE

  2. The screen will display some infomation. Press <Enter> .

  3. Responds to the screen prompts, selecting "Change Network
  Configuration",then press <Enter>.

  4. Move the highlight to "Add Adapter", press <Enter>.

  5. Select "Network adapter not shown on list below ...".

  6. Insert the DGE-528T driver diskette in floppy A,and
  specify your pathname A:\NDIS2\DOS ,then press <Enter>.

  7. Follow screen instructions to complete the process. Simply
  pressing <Enter> for each screen display will select the default
  options. Press <Enter> until you reach the display prompting you
  to reboot your system.


  Installing Multiple LAN Adapters:
  ---------------------------------
  There are two different method to complete it:

  To Follow Installation Procedure and add two adapter,

  (a) Under DOS mode, you can modify the EtherID or BusNo+DeviceNo
  keyword field in file C:\MSCLIENT\PROTOCOL.INI.

  (b) Or you can also use the SETUP program and follow above
  setup procedurc step 4,but move the highlight to "Change
  Setting,then press <Enter>, the screen will prompt you to
  fill EtherID value .

