  Windows 2000

  Introduction:
  -------------
  This document describes the procedure to install Windows 2000 driver
  for D-Link DGE-528T Gigabit Ethernet Adapter.

  Location of Windows 2000 Driver : \WIN2K\DLKRTGB.SYS

  Installing driver for Windows 2000:
  -----------------------------------
  Before you start with the installation process, make sure that your
  adapter should be properly installed in your PCI bus slot.
  Executing Windows 2000, it will auto-detect your system configuration and
  find the adapter hardware.
  (If Windows 2000 does not prompt that it detects the Ethernet Controller,
  there must be something wrong with the DGE-528T Gigabit Ethernet
  adapter or your system enviroment.)

  1. Ask you to select which driver you want to install, select "Search for
  a suitable driver for my device(recommended)".

  2. Insert the DGE-528T Windows driver disk into drive A and specify
  the setup file pathname A:\WIN2K after select "Specify a location".

  3. The Windows 2000 will start to copy the drivers into the system.

  4. Windows 2000 will finish the other installation procedure automatically.

