<Linux device driver for Realtek Ethernet controllers>

  This is the Linux device driver released for RealTek Ethernet controllers, which are listed as following.
	1. RTL8169S/SB/SC (Gigabit Ethernet with PCI interface)
	2. RTL8168B (Gigabit Ethernet with PCI-Express interface)
	3. RTL8101E (Fast Ethernet with PCI-Express interface)

<Requirements>

  - kernel source tree (supported versions 2.4.x or 2.6.x)
  - compiler/binutils for kernel compilation



<Quick install with proper kernel settings>

  Unpack the tarball :
	unzip r1000_linuxdrv_vxx.zip

  Change to the directory:
	cd r1000

  If you are running the target kernel, then you should be
  able to do :

	make clean modules	(as root or with sudo)
	make install
	depmod -a




<Force Media Speed>

 The media can be forced to one of the 5 modes as follows.

        Cmd: "insmod r1000 media = SET_MEDIA"
        For example:
         "insmod r1000 media = 0x04" will force PHY to operate in 100Mpbs Half-duplex.

         SET_MEDIA can be:
                _10_Half        = 0x01
                _10_Full        = 0x02
                _100_Half       = 0x04
                _100_Full       = 0x08
                _1000_Full      = 0x10


   Force media type for multiple cards could be performed as:

         "insmod r1000 media=0x04,0x10"

   which force PHY to operate at 100Mbps half-duplex and 1000Mbps full-duplex.



<Advanced feature>

  - Supports Jumbo Frame
  - Hardware Tx/Rx flow control

