Intel(R) PRO Network Connections Software Version 10.2 Release Notes
====================================================================

October 13, 2005

This release includes software and drivers for Intel(R) PRO/100 and
Intel(R) PRO/1000 adapters and integrated network connections.

Contents
========

- What's New in This Release
- Intel Fiber Optic Adapters
- Intel(R) PRO/1000 PM Network Connection Notes
- Microsoft Windows XP Notes
- Microsoft Windows 2000 Notes
- Intel(R) Quad Port Server Adapter Installation Notes
- Known Issues
- Customer Support


What's New in This Release
==========================

- Support for Enhanced ASPM power saving mode on systems with an
  Intel(R) PRO/1000 PL Network Connection


Intel Fiber Optic Adapters
==========================

Caution: The fiber optic ports may utilize Class 1 or Class 1M laser 
devices. Do not stare into the end of a fiber optic connector 
connected to a "live" system.  Do not use optical instruments to 
view the laser output. Using optical instruments increases eye hazard.  
Laser radiation is hazardous and may cause eye injury.  To inspect a 
connector, receptacle or adapter end, be sure that the fiber optic 
device or system is turned off, or the fiber cable is disconnected 
from the "live" system. 

The Intel PRO/1000 adapters with fiber optic connections
operate only at their native speed and only at full-duplex.  Therefore
you do not need to make any adjustments.  Use of controls or
adjustments or performance of procedures other than those specified
herein may result in hazardous radiation exposure.  The laser module 
contains no serviceable parts.  

Jumbo Frames
============

Some Intel gigabit adapters that support Jumbo Frames have a frame size limit 
of 9238 bytes, with a corresponding MTU size limit of 9216 bytes. The adapters 
with this limitation are based on the Intel 82571EB and 82572EI controllers, 
which also have these product names: 
 Intel PRO/1000 PT Server Adapter 
 Intel PRO/1000 PT Desktop Adapter 
 Intel PRO/1000 PF Server Adapter
 Intel PRO/1000 PT Dual Port Server Adapter
 Intel PRO/1000 PF Dual Port Server Adapter

The Intel PRO/1000 PM Network Connection and Intel PRO/1000 PL Network 
Connection do not support jumbo frames.


Microsoft Windows XP Notes
==========================

Microsoft Windows XP Known Issues
---------------------------------
  
  Error Disabling Connection
  --------------------------
  Disabling an adapter from Network Control Panel causes an error. Using 
  Device Manager to disable an adapter resolves this issue.

  TCP Segmentation Offload is not supported
  -----------------------------------------
  TCP Segmentation Offload (Large Send Offload) has performance issues with
  Windows XP due to Microsoft issues.  The feature is disabled by default 
  upon install and upgrade regardless of previous settings.  This is only
  for Windows XP and is for all versions and service packs of Windows XP.
  For more information reference MS Knowledge base article 842264. 


Microsoft Windows 2000 Notes
=============================

Service Pack 4 Required for Microsoft Windows 2000
--------------------------------------------------
Windows 2000 Service Pack 4 is required for Intel network drivers 
and software to function correctly.

Microsoft Windows 2000 Known Issues
-----------------------------------

  Error Disabling Connection
  --------------------------
  Disabling an adapter from Network Control Panel causes an error. Using 
  Device Manager to disable an adapter resolves this issue.

  Incorrect command line parameters when running DXSetup.exe
  ----------------------------------------------------------
  The version of Windows Installer in the base install of Windows 2000
  is out of date. Please update to version 3.0 or 3.1. They can be 
  found on the Microsoft website http://www.microsoft.com/downloads/


Intel Quad Port Server Adapter Notes
====================================

The Intel(R) PRO/1000 MT Quad Port Server Adapter operates in 3.3 volt 
PCI-X slots only. For best performance, this adapter should be installed 
in a 64-bit PCI-X slot. 

Hot Plug operations are not supported by Intel quad port server adapters.

Wake on LAN is not supported on the Intel PRO/1000 MT Quad Port Server 
Adapter.


Intel Quad Port Server Adapter Known Issues
-------------------------------------------

  Multiple Intel quad port adapters in one system
  -----------------------------------------------
  Installing more than two Intel quad port server adapters in the same 
  system is not recommended. Many systems are unable to support the power 
  requirements for more than two of these adapters. 

  Use only in a PCI-X Slot
  ------------------------
  Reduced performance has been observed when the Intel PRO/1000 MT Quad 
  Port Server Adapter is installed in a slot other than a PCI-X slot.

  Shared Interrupt Limitation 
  ---------------------------
  In some systems, the BIOS and OS assign the same interrupt number to 
  two or more different ports on the Intel PRO/1000 MT Quad Port Server 
  Adapter. If this occurs, these ports do not function properly. To 
  address this issue, reassign the system resources so that each port 
  of the adapter has its own unique interrupt number or disable one of 
  the ports sharing the same interrupt number. 

  Downshifting
  ------------
  When connecting to any Gigabit switch via a faulty CAT 5 cable where 
  one pair is broken, the adapter does not downshift from 1 Gig to 
  100Mbps. For the adapter to downshift, it must identify two broken 
  pairs in the cable.
  
  Installing the Base Driver on systems running Windows XP 
  or Windows Server 2003
  --------------------------------------------------------
  After inserting the adapter in the system, you must install the base
  driver. This is true even if you previously installed base drivers
  for other Intel Ethernet adapters.

  Intel PRO/1000 MT Quad Port Server Adapter Not recommended 
  for use on some systems
  ----------------------------------------------------------
  The Intel PRO/1000 MT Quad Port Server Adapter does not function 
  correctly in the following systems:
 
  Dell* PowerEdge* 2500
  Dell PowerEdge 6400
  Dell PowerEdge 6450
  Dell PowerEdge 6650SC
  Intel Saber, Saber-R, and Saber-Rx Systems
  SuperMicro* 370DE6
  SuperMicro P4DP6
  IBM* eServer* xSeries* 365
 
  Using the Intel PRO/1000 MT Quad Port Server Adapter in these 
  configurations is not recommended.

  Heavy traffic may cause system reboot in some systems
  -----------------------------------------------------
  Using an Intel PRO/1000 MT Quad Port Server Adapter may cause a reboot 
  in systems with the Intel Profusion chipset including: Intel OCPRF100 
  and SRPM8 server systems; Compaq* ProLiant* 8000, 8500, ML750, DL760; 
  Dell PowerEdge 8450, 6300, 6350; IBM* x370.  Using the Intel PRO/1000 
  MT Quad Port Server Adapter in these configurations is not recommended.


Known Issues
============

  Procedure for installing and upgrading drivers and utilities
  ------------------------------------------------------------
  Intel does not recommend installing or upgrading drivers and Intel(R)
  PROSet software over a network connection. Instead, install or upgrade
  drivers and utilities from each system. 

  Windows Code 10 Error Message on Driver Install or Upgrade
  ----------------------------------------------------------
  If you encounter a Windows Code 10 error message when installing or 
  upgrading drivers, reboot to resolve the issue.

  Throughput reduction after Hot-Replace
  --------------------------------------
  If an Intel gigabit adapter is under extreme stress and is hot-swapped,
  throughput may significantly drop.  This may be due to the PCI property
  configuration by the Hot-Plug software.  If this occurs, throughput can
  be restored by restarting the system.

  Intel PRO Adapters ignore consecutive Wake Up signals while
  transitioning into standby mode
  -----------------------------------------------------------
  While sending a system into standby, occasionally a wake up packet 
  arrives before the system completes the transition into standby mode.
  When this happens, the system ignores consecutive wake up signals
  and remains in standby mode until manually powered up using the
  mouse, keyboard, or power button.

  Link Difficulties With 82541 or 82547 Based Connections
  -------------------------------------------------------
  The PROSet Advanced tab now contains a setting allowing the 
  master/slave mode to be forced. This improves time-to-link with 
  some unmanaged switches. For older adapters and controllers, you 
  may encounter difficulty with 82541 or 82547 based connections.

  Intel PRO/1000 Adapters (copper only) do not detect active link 
  during load time
  ---------------------------------------------------------------
  Some Intel PRO/1000 adapters, especially copper adapters, cannot
  detect an active link during load time. To resolve this issue, try
  the following workarounds.
  - Re-attach to the server without reloading the driver.
  - For DOS-based installations, add a delay of 4 to 5 seconds in the 
    batch file after the load driver command.
  - Load the configuration by manually entering commands.
  - Set adapter to link at 1000 Mbps only. 


Customer Support
================

- Main Intel web support site: http://support.intel.com

- Network products information: http://www.intel.com/network

- Worldwide access: Intel has technical support centers worldwide.  Many of
  the centers are staffed by technicians who speak the local languages. For
  a list of all Intel support centers, the telephone numbers, and the times
  they are open, visit http://www.intel.com/support/9089.htm.

- Telephone support: US and Canada: 1-916-377-7000 
  (07:00 - 17:00 M-F Pacific Time) 


Legal / Disclaimers
===================

Copyright (C) 1998-2005, Intel Corporation.  All rights reserved.

Intel Corporation assumes no responsibility for errors or omissions in 
this document. Nor does Intel make any commitment to update the information 
contained herein.

* Other product and corporate names may be trademarks of other companies 
and are used only for explanation and to the owners' benefit, without intent 
to infringe.
