
  << About the re-installation of the driver at the time of problem >>

    In PC without a local port (LPT1,COM1 etc.),
    setup error occurs during driver installing,
    or port write error occurs at the time of FAX transmission.
    In that case, please re-install the driver,
    according to the installation procedure below.

[ Installation procedure ]

1. Delete the FAX Driver already installed.

2. Start up the driver installer.

      Double-Click the "<CD-ROM:>\FAX\FAXDRV\FAXDriver\KMSetup.exe" to start up the driver installer.

3. The wizard screen of "Select a device port" is displayed while installing it.
   Please select the "Create a new port", select "Port Set Up Port" from the type menu, and click
   "Next" button on the wizard screen. 

4. The "Add Port Wizard" will start up and continue the Wizard selecting the "Print using Raw mode".
   Please input "IP Address or Host Name" IP Address of NetworkFAX address.

      *** Caution ***
        You must input NetworkFAX address with IP Address, not Host Name.


