**
**
**  D-Link DFE-520TX PCI Fast Ethernet Adapter
**
**  NDIS Driver for LANTASTIC
**
**  v4.38    Feb  , 2007
**
**

Introduction:
=============

  This document shows you how to install Lantastic NDIS driver
  and how to use the enhanced functions by setting the custom keywords.


Contents of the Subdirectory:
=============================

    LANTASTI.TXT        This file.
    DLKFET.DOS          The NDIS2 driver.
    PROTOCOL.INI        Sample protocol.ini file.



Installation:
=============

  Before starting with the installation process, make sure that the adapter
  is properly installed and configured. You can use the diagnostic program
  (DIAG.EXE) to make sure your connection with the network is correct.

  Install procedure for Lantastic 6.0
  -----------------------------------

    1) Run Lantastic 6.0 install program and follow screen instructions.

    2) When the "Network Adapter Setup" appears, Select "Use NDIS driver for
       non-Artisoft adapter" and type "A:\LANTASTI" in the search path and
       select "Search" button.

    3) When the install program find FETND NDIS driver, select "OK" to continue.

    4) Follow the screen instructions to complete the installation.

    5) Restart the computer.

  Manual install for Lantastic 6.0/5.0
  ------------------------------------

    You can replace the NDIS driver by modify the following configuration files:

        Sample CONFIG.SYS
        -----------------

        DEVICE=C:\LANTASTI\PROTMAN.DOS /I:C:\LANTASTI
        DEVICE=C:\LANTASTI\DLKFET.DOS


        Sample STARTNET.BAT
        -------------------

        C:\LANTASTI\AI-NDIS BIND_TO=FETND_NIF
        C:\LANTASTI\AILANBIO


        Sample PROTOCOL.INI
        -------------------

        [PROTMAN]
           DRIVERNAME = PROTMAN$
           DYNAMIC = YES

        [FETND_NIF]
           DRIVERNAME = DLKFET$


Configuration Files:
====================

    You can change the configuration by modify PROTOCOL.INI file.

    File Name:          PROTOCOL.INI
    ----------
    Sample of configuration file:
    -----------------------------

        ...
        [FETND_NIF]
        DRIVERNAME=DLKFET$
      
        ...


    Custom Keywords:
    ----------------
        FULLDUPLEX                      This keyword is used to enable full
                                        duplex mode.
                                        (suggest use CONNECTIONTYPE instead of this keyword)

        SPEED                           This keyword is used to force the
	                                    adapter at 10Mbps or 100Mbps speed.
                                        (suggest use CONNECTIONTYPE instead of this keyword)

        AUTO                            This keyword is used to force the
                                        chip at Auto-Negotiation mode.
                                        (suggest use CONNECTIONTYPE instead of this keyword)

        DEVICENO                        This keyword is used to force device number
                                        for specified NIC card


        BUSNO                           This keyword is used to force bus number for
                                        specified NIC card

        CONNECTIONTYPE                  This keyword is used to specify duplex 
                                        and speed mode. The strings are :
                                        
                                        AUTOSENSE
                                        _10BaseT  
                                        _10BaseTFD
                                        _100BaseTX   
                                        _100BaseTXFD 
                                        
        FLOWCTRL                        This keyword is used to specify flow contro
                                        ability. The strings are :
                                        
                                        HARDWARE_DEFAULT (Auto Mode)
                                        ENABLE
                                        DISABLE

                                        Driver doesn't care the result of auto-negotiate if 
                                        the value of this keyword, FLOWCTRL , is ENALBE or
                                        DISABLE. It just enables or disable flow control
                                        ability according your setting.

        NETWORKADDRESS                  This keyword is used to override the network address
                                        of the network adapter. Its type is :
                                        
                                        "000123456789"


        Note: If you want to specify NIC card, the DEVICENO is necessary, but BUSNO is optional
              When the NIC cards in the system have the same device number, you can use 
              BUSNO to specify.
              If there are two or more NIC cards in the system and you don't specify anyone,
              driver will display the menu for selection. You can get the information about 
              bus number and device number form this menu.
                                        